Index: gkrellm-2.3.1/server/gkrellmd.conf
===================================================================
--- gkrellm-2.3.1.orig/server/gkrellmd.conf	2008-03-09 10:19:26.000000000 +0100
+++ gkrellm-2.3.1/server/gkrellmd.conf	2008-03-09 10:19:26.000000000 +0100
@@ -4,7 +4,7 @@
 # the client update frequency.  Values may be from 1 to 10 and should be
 # smaller values to reduce network traffic.
 #
-update-hz 3
+update-hz 10
 
 # Limit number of simultaneous clients allowed to connect.
 #
@@ -13,7 +13,7 @@
 # Specify a specific network interface to listen on for connections.
 # By default gkrellmd listens on all available network interfaces.
 #
-address 127.0.0.1
+#address 127.0.0.1
 
 # Specify the port to listen on for connections.
 #
@@ -29,14 +29,14 @@
 
 # Drop privileges after startup (you must start gkrellmd as root to do it).
 #
-#user	nobody
+user	nobody
 #group	proc
 
 # Create a PID file for the running gkrellmd.  Default is no PID file.
-#pidfile /var/run/gkrellmd.pid
+pidfile /var/run/gkrellmd.pid
 
 # Run in background and detach from the controlling terminal
-#detach
+detach
 
 # Time interval between checks for various monitors.  If nfs-interval
 # is <= 0 then gkrellmd will not read data for nfs file system types.
